**SP-XX 6” CONCRETE WHEELCHAIR RAMPS**

Version Date: 11/30/2018 Revision Date: XX/XX/XXXX by XXX

**1.0 DESCRIPTION**

The work covered by this special provision includes all work covered in Section 848 of the NCDOT Standard Specifications “Concrete Sidewalks and Driveways and Wheelchair Ramps”. The concrete wheelchair ramps shall be constructed in accordance with the detail drawings and specifications, at locations indicated in the plans. Truncated domes shall be included and installed per NCDOT Std No. 848.05. Proposed wheelchair ramps may vary from details in order to conform to existing conditions but must meet American with Disabilities Act (ADA) and Accessibility Guidelines for Pedestrian Facilities in the Public Right-of-Way (PROWAG) requirements.

2.0 MATERIALS

All materials shall be in accordance with section 848 of the NCDOT Standard Specifications and detail 848.05 of the NCDOT Roadway Standard Drawings.

**3.0 MEASUREMENT**

The quantity of wheelchair ramps to be paid for will be the actual number of square yards of wheelchair ramps, measured along the surface of the completed work which has been completed and accepted. There will be no separate measurement for truncated domes. The vertical curb associated with the directional ramps will be included in the square yard measurement.

**4.0 PAYMENT**

The quantity of wheelchair ramps, measured as provided above, will be paid for at the contract unit price per square yard for “6" Concrete Wheelchair Ramps”. There will be no other pay items in this provision. All costs for labor, equipment, and materials necessary to complete this provision (including truncated domes) will be included in the price bid for 6" Concrete Wheelchair Ramps. Payment will be made separately at the contract unit prices for the curb and gutter adjacent to the roadway pavement for the various curb types in NCDOT Section 846.

Payment will be made under:

**6” CONCRETE WHEELCHAIR RAMPS SY**