**SP-XX 6” Concrete Multi-Use Path (MUP)**

Version Date: 9/13/2019 Revision Date: XX/XX/XXXX by XXX

**1.0 DESCRIPTION**

The work covered by this special provision includes the construction of 6” Concrete multi-use path (MUP) in accordance with Charlotte Land Development Standard 10.42, as shown in the plans and as covered in Section 848 of the 2018 NCDOT Standard Specifications “Concrete Sidewalks, Driveways and Curb Ramps.”

2.0 MATERIALS

Concrete shall be at least 3600 PSI compressive strength and all materials shall be in accordance with Charlotte Land Development Standard 10.42 and section 848 of the 2018 NCDOT Standard Specifications.

**3.0 MEASUREMENT**

The quantity of 6” Concrete MUP to be paid for will be the actual number of square yards of 6” concrete multi-use path, measured along the surface of the walk that has been constructed and accepted.

**4.0 PAYMENT**

Payment for 6” Concrete MUP, measured as stated above, will be paid for at the contract unit price for “6” CONCRETE MULTI-USE PATH (MUP).” There will be no separate payment for materials, labor, equipment, and other incidentals necessary to complete the work including sawcut joints and sealing joints. Such payment will be full compensation for all work covered by this special provision and includes all labor, equipment, and materials necessary to complete the work as specified. If aggregate base course is needed per CLDS 10.42, this will be paid for separately.

Payment will be made under:

**6” CONCRETE MULTI-USE PATH (MUP) SY**