## SP-XX, PEDESTRIAN BRIDGE

Version Date: 6/1/2018 Revision Date: XX/XX/XXXX by XXX

### DESCRIPTION

Work covered in this special provision includes installation of pedestrian bridges as shown on the civil plans and structural details. The addresses where pedestrian bridges will be installed are identified below:

* [ADDRESS #1]
* [ADDRESS #2]

### CONSTRUCTION METHODS AND MATERIALS

All materials and installation shall be in accordance with the structural details and notes provided on plan sheets, S-X, and S-X.

### MEASUREMENT

Pedestrian bridges will be measured by square foot of surface area for each address upon completion and acceptance by the Engineer

### PAYMENT

Payment shall include but not be limited to all timber, metal, decking, rails, top caps, struts, posts, bracing, stringers, sleepers, ledges, blocking, anchors, plates, angles, clips, bolts, washers, screws, nails, piers, concrete, reinforcing steel, welding, and other necessary hardware, materials, labor and equipment necessary to complete the work shown on the plans. Excavation and backfill shall be as specified in the Earthwork, Excavation, Unsuitable Materials, and Backfill Materials special provision.

Payment will be made under:

**PEDESTRIAN BRIDGE, TIMBER SF**

**PEDESTRIAN BRIDGE, STEEL SF**