#### SP-XX, Reset Existing Frame and Grates/Covers

Version Date: 11/13/2018 Revision Date: MM/DD/YYYY by XXX

**1.0 DESCRIPTION**

Work covered by this special provision consists of removing and resetting existing frame and grates or ring and covers as shown on the plans or as directed by the Engineer and in accordance with the provisions of these specifications.

**2.0 MATERIALS**

The Engineer will inspect the existing frame and grates or ring and covers. The Contractor will be instructed to reuse frame and grates or ring and covers as directed by the Engineer.

**3.0 CONSTRUCTION** **METHODS**

Construction methods for frame and grates or ring and covers shall be in accordance with 840 "Minor Drainage Structures" of the North Carolina Department of Transportation Standard Specifications and the manufacturers’ recommendations. Remove with caution to avoid damaging the items from the existing state. Contractor shall store in a safe place until ready to reset. Reset the frame, grates, ring and/or covers in a condition equal to or better than what was removed.

**4.0 MEASUREMENT**

The quantity for reset existing frames and grates/covers will be measured on a per each basis for each frame and grate/cover that can be reused in the completed and accepted work.

**5.0 PAYMENT**

The quantity for reset existing frames and grates/covers, measured as provided above, will be paid for at the contract unit price per each for "Reset Existing Frame and Grates/Covers (All Types)". Such payment will be full compensation for all work of removing, storing, and resetting the existing frame and grate/cover onto the new or existing structure. There will be no compensation for any items damaged by the Contractor’s forces.

Payment will be made under:

**Reset Existing Frame and Grates/Covers (All Types)……………………………………………………………..………………… EA**