**SP-XXX SAFETY RAIL, METAL CLDS 50.04**

Version Date: 12/11/2015 Revision Date: XX/XX/XXXX by XXX

**1.0 DESCRIPTION**

The work covered by this special provision includes furnishing all materials, labor, equipment, and incidentals necessary to install painted metal handrails in accordance with these provisions, Charlotte Land Development Standard (CLDS) 50.04 detail drawings, and the plans at locations identified in the plans and as directed by the Engineer.

**2.0 MATERIALS**

All materials for the safety rail shall comply with CLDS 50.04.

3.0 MEASUREMENT

The quantity of metal safety rail to be paid for will be the actual number of linear feet of safety rail, measured along the top bar of the rail, which has been installed and accepted.

4.0 PAYMENT

Metal handrail will be paid for at the contract unit price per linear foot for "Safety Rail, Metal CLDS 50.04". Such payment will be full compensation for all work covered by this special provision, including but not limited to fabricating, furnishing, delivering, and installing the handrail; furnishing paint and painting the handrail; all excavation and backfilling, and furnishing and placing concrete footings; all materials, labor, and equipment necessary to complete the work.

Payment will be made under:

**SAFETY RAIL, METAL CLDS 50.04 LF**