#### SP-XX, SPLIT RAIL FENCE

Version Date: 5/19/2021 Revision Date: MM/DD/YYYY by XXX

**1.0 DESCRIPTION**

The work covered by this special provision consists of furnishing and erecting split rail fence as indicated on the work order and as directed by the Engineer.

**2.0 MATERIALS**

Posts: All material for timber posts and braces shall meet the requirements of Section 866-2 “Materials” of the Standard Specifications.

**3.0 CONSTRUCTION METHODS**

Construction methods for split rail fence shall be in accordance with manufacturers’ specifications. For split rail fence with wire, the wire fabric will be securely fastened to the split rail fence and the split rail gate with fasteners indicated by the manufacturer or as directed by the Engineer. Split rail gates must be approved by the Engineer.

**4.0 MEASUREMENT**

Split Rail Fence: The quantity of split rail fence will be measured in linear feet of split rail fence, measured in place from center of each post or gate post to center of end post or gate post exclusive of gate sections, which has been completed and accepted.

Gates: The quantity of gates will be measured in units of each for the number of gates actually erected which have been installed and accepted.

Wire Fabric: The quantity of wire fabric will be measured in linear feet of wire fabric, which has been installed and accepted.

There will be no separate measurement for timber rails, posts, braces, fasteners and incidental materials required to complete the split rail fence as directed by the Engineer.

**5.0 PAYMENT**

Split Rail Fence: The quantity of split rail fence will be paid in linear feet of split rail fence, quantified per Section 4.0 Measurement.

Gates: The quantity of gates will be paid in units of each for the number of gates actually erected which have been installed and accepted.

Wire Fabric: The quantity of wire fabric will be paid in linear feet of wire fabric, which has been installed and accepted.

There will be no separate payment for timber rails, posts, braces, fasteners and incidental materials required to complete the split rail fence as directed by the Engineer.

Such prices and payments will be full compensation for all elements of work required to furnish and install proposed fence, rails, posts, braces, fasteners and all incidentals necessary to complete the split rail fence as directed by the Engineer.

Payment will be made under:

**4’ SPLIT RAIL FENCE (2-Rail) LF**

**4’ SPLIT RAIL FENCE (3-Rail) LF**

**2″ X 4″ WIRE FABRIC LF**

**4’ SPLIT RAIL FENCE (Standard Gate) EA**

**4’ SPLIT RAIL FENCE (Standard Gate Reset) EA**