**SP-XXX PEDESTRIAN REFUGE ISLAND (PASS-THRU)**

Version Date: 12/11/2015

 Revision Date: XX/XX/XXXX by XXX

1. **DESCRIPTION**

The work covered by this special provision includes all elements of work covered by section 848, “Concrete Sidewalks, Driveways and Wheel Chair Ramps” of the NCDOT Standard Specifications and the detail for the Pedestrian Refuge Island (Pass-Thru) as shown on the plans. Truncated domes shall be included and installed per NCDOT Std No. 848.05.

1. **MATERIALS**

All materials shall be in accordance with section 848 of the NCDOT Standard Specifications and detail 848.05 of the NCDOT Roadway Standard Drawings.

1. **MEASUREMENT**

The quantity of Pedestrian Refuge Island (Pass-Thru) to be paid for will be the actual number of square yards completed and accepted. There will be no separate measurement of wheelchair ramps or truncated domes. Any concrete slope tie-ins between the pedestrian island cap, monolithic concrete, or planting mix and the pass thru will be paid for under this item and measured in square yards. Any curb required adjacent to the pedestrian refuge island (pass-thru) will be measured by the appropriate curb line item in the contract.

1. **PAYMENT**

Payment for the Pedestrian Refuge Island (Pass-Thru) as measured above shall be paid for at the contract unit price for “Pedestrian Refuge Island (Pass-Thru)”. Such payment shall include all labor, equipment and materials required to construct the pass-thru necessary to complete this provision, including truncated domes will be included in the price bid for Pedestrian Refuge Island (Pass thru). Any curb required adjacent to the pedestrian refuge island (pass-thru) will be paid by the appropriate curb line item in the contract.

Payment will be made under:

**PEDESTRIAN REFUGE ISLAND (PASS-THRU)…………………………………………………………………………………SY**