**SP-XX, TEMPORARY PET CONTAINMENT FENCE**

Version Date: 11/2/2017 Revision Date: MM/DD/YYYY by XXX

1. **Description:**

The work covered by this section consists of furnishing, installing, maintaining, and removing temporary pet containment fence. The quantity of temporary pet containment fence to be installed will be affected by the actual conditions which occur during the construction of the project. The installation may require gates at the direction of the inspector. The quantity of temporary pet containment fence may be increased or decreased at the direction of the Engineer. Such variations in quantity will not be considered as alterations in the details of construction or a change in the character of the work.

1. **Materials:**

Reuse of temporary pet fencing materials is encouraged. When there is no opportunity to repurpose temporary pet fence materials, new materials shall be utilized. Acceptance is subject to suitable functionality. On properties where wire fence exists, wire fence for temporary pet containment shall have openings no larger than the existing fence.

1. **Measurement:**

Measurement will be the actual linear feet of temporary pet containment fence installed. There will be no separate measurement for gates or posts.

1. **Payment:**

The quantity of fence will be paid for at the contract unit price per linear foot for “Temporary Pet Containment Fence.” Such payment will be full compensation for all materials, labor and incidentals. There will be no separate payment for gates or posts.

Payment will be made under:

**TEMPORARY 4 FT. PET CONTAINMENT FENCE............................................................................... LF**

**TEMPORARY 6 FT. PET CONTAINMENT FENCE............................................................................... LF**