#### SP-XX, WOOD PRIVACY FENCE

Version Date: 5/19/2021 Revision Date: MM/DD/YYYY by XXX

**1.0 DESCRIPTION**

Work covered by this special provision consists of furnishing and erecting wood link fence as shown on the plans and in accordance with the provisions of these specifications.

**2.0 MATERIALS**

The material will be wood with wood posts to match the existing wood privacy fence. The Contractor will inspect the existing fence to determine the materials and replace to match original.

The gates shall match the existing material. The Contractor will inspect the existing fence and gates that are to be replaced and restore to original specifications.

**3.0 CONSTRUCTION** **METHODS**

Construction methods for wood link fence shall be in accordance with 866 "FENCE" of the NCDOT Standard Specifications and the manufacturers’ recommendations.

Work covered by this special provision consists of work described in section 866 "FENCE" of the NCDOT Standard Specifications and the following sub-articles: 866-2 Materials, 866-3 Construction Methods.

**4.0 MEASUREMENT**

The quantity of wooden fence to be measured will be the actual number of linear feet of fence, measured from center of post to center of post, which has been completed and accepted. The quantity of gates to be measured will be per each gate which has been completed and accepted. There will be no separate measurement of posts.

**5.0 PAYMENT**

The quantity of wooden fence, measured as provided above, will be paid for at the contract unit price per linear foot for "Fence, Wooden". Such payment will be full compensation for all work of furnishing and installing proposed fence to include but not limited to terminal posts, line posts, top rails, and all incidental materials. The quantity of gates to be paid for will be per each gate which has been completed and accepted. There will be no separate payment of posts.

Payment will be made under:

**FENCE, 4’ WOOD PRIVACY FENCE ……………………………………………………………………………………..………………… LF**

**FENCE, 4’ WOOD (GATE)...………………………………………………………………………………………………………………..… EA**

**FENCE, 5’ WOOD PRIVACY FENCE …………………………………………………………………………………….………………… LF**

**FENCE, 5’ WOOD (GATE)……....………………………………………………………………………….……………………………..… EA**

**FENCE, 6’ WOOD PRIVACY FENCE …………………………………………………………………………………….………………… LF**

**FENCE, 6’ WOOD (GATE)….....………………………………………………………………………….………………………………..… EA**