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1. DESCRIPTION

The work covered by this special provision consists of furnishing, installing, maintaining, and removing temporary pet containment fence and gates(where applicable) as shown on the plans or as directed by the engineer. 

1. MATERIALS

Temporary pet containment fence shall provide an equal or greater level of containment as the existing fence.  At a minimum, fence materials shall be a type that is flexible and secure, allowing for movement without undue damage.  Post shall be installed at an adequate spacing to provide the required level of containment but at no point shall spacing exceed 16’ between posts. 
Where temporary pet containment fencing is installed:
· If an existing wire fence is present, the temporary fence openings shall be no larger than those of the existing fence.
· If no existing wire fence is present, the fence material shall have openings no greater than 2” x 4”.
Reuse of materials is permitted and encouraged, provided they are free of deterioration or damage that could compromise containment.


1. MEASUREMENT

Measurement will be based on the actual linear feet of temporary pet containment fence installed, with no separate measurement for gates or posts.

The quantity may be increased or decreased at the direction of the Engineer. Such adjustments will not be considered a change in the character of the work or an alteration of construction details.

The final installed quantity will depend on actual field conditions encountered during construction.


1. PAYMENT

The quantity of fence will be paid for at the contract unit price per linear foot for “Temporary Pet Containment Fence.” Such payment will be full compensation for all materials, labor, equipment and incidentals. There will be no separate payment for gates or posts.

Payment will be made under:

TEMPORARY 4 FT. PET CONTAINMENT FENCE......................................................................................................LF
TEMPORARY 6 FT. PET CONTAINMENT FENCE......................................................................................................LF


